**Brown-Nassau Instructions**

1. Select correct side and Vernia
2. Pencil mark Lat and LHA on correct baseplate
3. Set Dec on correct Vernia
4. Read Hc from 2 mark position among alt curves on rotor.
5. Select side for Az
6. Set Hc on correct Vernia
7. Dec point rotor/lat point baseplate, extend down to Az bottom baseplate.